

**Chisel Usable Limit.**

Please check Chisel length after pulling out chisel from hammer without taking off Retainer Pin.

A: New chisel length.

|  |  |  |
| --- | --- | --- |
| Model | A ( New Chisel length ) | B ( Usable Chisel Limit) |
| GH-9 | 618 mm | 336 mm |

B: Usable limit length.

Over all GH-9 Chisel Length is 1200 mm

Please fill the following details from different job sites:

Model : GH-9 / GH(S)-9

Serial Number :\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

|  |  |  |
| --- | --- | --- |
| **Rock Type** | Number of Hours | A’  (Chisel Length remaining after usage )-mm |
| **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_** | \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |